<circuit type="simulide_1.0" stepSize="1000000" stepsPS="1000000" NLsteps="100000" animate="0" >

<item itemtype="Subcircuit" CircId="Uno-1" mainComp="false" Show_id="true" Show_Val="false" Pos="-284,-244" rotation="0" hflip="1" vflip="1" label="Arduino Uno" idLabPos="54,-24" labelrot="0" valLabPos="0,0" valLabRot="0" Logic_Symbol="false">
<mainCompProps itemtype="MCU" CircId="1_mega328-109" mainComp="true" Show_id="false" Show_Val="false" Pos="20,20" rotation="0" hflip="1" vflip="1" label="1_mega328-109" idLabPos="0,-20" labelrot="0" valLabPos="-16,20" valLabRot="0" Frequency="16 MHz" Program="pcd-spi-h.hex" Auto_Load="false" Rst_enabled="true" Ext_Osc="true" Wdt_enabled="false" />
</item>

<item itemtype="Pcd8544" CircId="Pcd8544-2" mainComp="false" Show_id="false" Show_Val="false" Pos="-372,-300" rotation="0" hflip="1" vflip="1" label="Pcd8544-2" idLabPos="-16,-24" labelrot="0" valLabPos="0,0" valLabRot="0" />

<item itemtype="Connector" uid="Connector-3" startpinid="Pcd8544-2-PinRst" endpinid="Uno-1-3" pointList="-404,-260,-404,-204,-276,-204" />

<item itemtype="Connector" uid="Connector-5" startpinid="Pcd8544-2-PinCs" endpinid="Uno-1-4" pointList="-388,-260,-388,-196,-276,-196" />

<item itemtype="Connector" uid="Connector-7" startpinid="Pcd8544-2-PinDc" endpinid="Uno-1-5" pointList="-372,-260,-372,-188,-276,-188" />

<item itemtype="Connector" uid="Connector-11" startpinid="Pcd8544-2-PinScl" endpinid="Uno-1-13" pointList="-340,-260,-340,-116,-276,-116" />

<item itemtype="Connector" uid="Connector-9" startpinid="Pcd8544-2-PinSi" endpinid="Uno-1-11" pointList="-356,-260,-356,-132,-276,-132" />

</circuit>