<circuit type="simulide_1.0" stepSize="1000000" stepsPS="1000000" NLsteps="100000" animate="0" >

<item itemtype="Fixed Voltage" CircId="Fixed Voltage-1" mainComp="false" Show_id="true" Show_Val="false" Pos="-612,-132" rotation="0" hflip="1" vflip="1" label="!Clear" idLabPos="-62,-7" labelrot="0" valLabPos="-16,8" valLabRot="0" Out="true" Voltage="5 V" />

<item itemtype="Fixed Voltage" CircId="Fixed Voltage-2" mainComp="false" Show_id="true" Show_Val="false" Pos="-612,-164" rotation="0" hflip="1" vflip="1" label="Serial / !Parallel Load" idLabPos="-112,-7" labelrot="0" valLabPos="-16,8" valLabRot="0" Out="true" Voltage="5 V" />

<item itemtype="Fixed Voltage" CircId="Fixed Voltage-3" mainComp="false" Show_id="true" Show_Val="false" Pos="-612,-196" rotation="0" hflip="1" vflip="1" label="Clock inhibit" idLabPos="-93,-7" labelrot="0" valLabPos="-16,8" valLabRot="0" Out="false" Voltage="5 V" />

<item itemtype="Fixed Voltage" CircId="Fixed Voltage-4" mainComp="false" Show_id="true" Show_Val="false" Pos="-612,-212" rotation="0" hflip="1" vflip="1" label="Clock" idLabPos="-62,-8" labelrot="0" valLabPos="-16,8" valLabRot="0" Out="true" Voltage="5 V" />

<item itemtype="Fixed Voltage" CircId="Fixed Voltage-5" mainComp="false" Show_id="true" Show_Val="false" Pos="-604,-292" rotation="0" hflip="1" vflip="1" label="E" idLabPos="-42,-7" labelrot="0" valLabPos="-16,8" valLabRot="0" Out="true" Voltage="5 V" />

<item itemtype="Fixed Voltage" CircId="Fixed Voltage-6" mainComp="false" Show_id="true" Show_Val="false" Pos="-604,-276" rotation="0" hflip="1" vflip="1" label="F" idLabPos="-42,-7" labelrot="0" valLabPos="-16,8" valLabRot="0" Out="false" Voltage="5 V" />

<item itemtype="Fixed Voltage" CircId="Fixed Voltage-7" mainComp="false" Show_id="true" Show_Val="false" Pos="-604,-244" rotation="0" hflip="1" vflip="1" label="H" idLabPos="-42,-7" labelrot="0" valLabPos="-16,8" valLabRot="0" Out="false" Voltage="5 V" />

<item itemtype="Fixed Voltage" CircId="Fixed Voltage-8" mainComp="false" Show_id="true" Show_Val="false" Pos="-604,-260" rotation="0" hflip="1" vflip="1" label="G" idLabPos="-42,-7" labelrot="0" valLabPos="-16,8" valLabRot="0" Out="true" Voltage="5 V" />

<item itemtype="Fixed Voltage" CircId="Fixed Voltage-9" mainComp="false" Show_id="true" Show_Val="false" Pos="-604,-324" rotation="0" hflip="1" vflip="1" label="C" idLabPos="-42,-7" labelrot="0" valLabPos="-16,8" valLabRot="0" Out="true" Voltage="5 V" />

<item itemtype="Fixed Voltage" CircId="Fixed Voltage-10" mainComp="false" Show_id="true" Show_Val="false" Pos="-604,-308" rotation="0" hflip="1" vflip="1" label="D" idLabPos="-42,-7" labelrot="0" valLabPos="-16,8" valLabRot="0" Out="false" Voltage="5 V" />

<item itemtype="Subcircuit" CircId="74XX166-11" mainComp="false" Show_id="true" Show_Val="false" Pos="-452,-428" rotation="0" hflip="1" vflip="1" label="74XX166-1" idLabPos="0,-20" labelrot="0" valLabPos="0,0" valLabRot="0" Logic_Symbol="false" />

<item itemtype="Subcircuit" CircId="74XX166-12" mainComp="false" Show_id="true" Show_Val="false" Pos="-500,-316" rotation="0" hflip="1" vflip="1" label="74XX166-1" idLabPos="0,-20" labelrot="0" valLabPos="13,72" valLabRot="-90" Logic_Symbol="true" />

<item itemtype="Probe" CircId="Probe-13" mainComp="false" Show_id="false" Show_Val="true" Pos="-396,-324" rotation="-45" hflip="1" vflip="1" label="Probe-3" idLabPos="16,-16" labelrot="45" valLabPos="16,0" valLabRot="45" ShowVolt="true" Threshold="2.5 V" />

<item itemtype="Fixed Voltage" CircId="Fixed Voltage-14" mainComp="false" Show_id="true" Show_Val="false" Pos="-604,-356" rotation="0" hflip="1" vflip="1" label="A" idLabPos="-42,-7" labelrot="0" valLabPos="-16,8" valLabRot="0" Out="true" Voltage="5 V" />

<item itemtype="Fixed Voltage" CircId="Fixed Voltage-15" mainComp="false" Show_id="true" Show_Val="false" Pos="-604,-340" rotation="0" hflip="1" vflip="1" label="B" idLabPos="-42,-7" labelrot="0" valLabPos="-16,8" valLabRot="0" Out="false" Voltage="5 V" />

<item itemtype="Fixed Voltage" CircId="Fixed Voltage-44" mainComp="false" Show_id="true" Show_Val="false" Pos="-604,-388" rotation="0" hflip="1" vflip="1" label="Serial IN" idLabPos="-74,-7" labelrot="0" valLabPos="-16,8" valLabRot="0" Out="false" Voltage="5 V" />

<item itemtype="Connector" uid="Connector-16" startpinid="Probe-13-inpin" endpinid="74XX166-12-QH" pointList="-412,-308,-412,-252,-460,-252" />

<item itemtype="Connector" uid="Connector-18" startpinid="Fixed Voltage-7-outnod" endpinid="74XX166-12-H" pointList="-588,-244,-508,-244" />

<item itemtype="Connector" uid="Connector-20" startpinid="Fixed Voltage-8-outnod" endpinid="74XX166-12-G" pointList="-588,-260,-572,-260,-572,-252,-508,-252" />

<item itemtype="Connector" uid="Connector-22" startpinid="Fixed Voltage-6-outnod" endpinid="74XX166-12-F" pointList="-588,-276,-564,-276,-564,-260,-508,-260" />

<item itemtype="Connector" uid="Connector-24" startpinid="Fixed Voltage-5-outnod" endpinid="74XX166-12-E" pointList="-588,-292,-556,-292,-556,-268,-508,-268" />

<item itemtype="Connector" uid="Connector-26" startpinid="Fixed Voltage-10-outnod" endpinid="74XX166-12-D" pointList="-588,-308,-548,-308,-548,-276,-508,-276" />

<item itemtype="Connector" uid="Connector-28" startpinid="Fixed Voltage-9-outnod" endpinid="74XX166-12-C" pointList="-588,-324,-540,-324,-540,-284,-508,-284" />

<item itemtype="Connector" uid="Connector-30" startpinid="Fixed Voltage-15-outnod" endpinid="74XX166-12-B" pointList="-588,-340,-532,-340,-532,-292,-508,-292" />

<item itemtype="Connector" uid="Connector-32" startpinid="Fixed Voltage-14-outnod" endpinid="74XX166-12-A" pointList="-588,-356,-524,-356,-524,-300,-508,-300" />

<item itemtype="Connector" uid="Connector-34" startpinid="Fixed Voltage-4-outnod" endpinid="74XX166-12-CLK" pointList="-596,-212,-556,-212,-556,-228,-508,-228" />

<item itemtype="Connector" uid="Connector-36" startpinid="Fixed Voltage-3-outnod" endpinid="74XX166-12-CINH" pointList="-596,-196,-548,-196,-548,-220,-508,-220" />

<item itemtype="Connector" uid="Connector-38" startpinid="Fixed Voltage-2-outnod" endpinid="74XX166-12-S/!LD" pointList="-596,-164,-540,-164,-540,-212,-508,-212" />

<item itemtype="Connector" uid="Connector-40" startpinid="Fixed Voltage-1-outnod" endpinid="74XX166-12-!CLR" pointList="-596,-132,-524,-132,-524,-204,-508,-204" />

<item itemtype="Connector" uid="Connector-45" startpinid="Fixed Voltage-44-outnod" endpinid="74XX166-12-SER" pointList="-588,-388,-516,-388,-516,-308,-508,-308" />

</circuit>