<circuit type="simulide_1.0" stepSize="1000000" stepsPS="1000000" NLsteps="100000" animate="1" >

<item itemtype="Subcircuit" CircId="74XX57-1" mainComp="false" Show_id="true" Show_Val="false" Pos="-404,-312" rotation="0" hflip="1" vflip="1" label="74XX57-1" idLabPos="0,-20" labelrot="0" valLabPos="13,26" valLabRot="-90" Logic_Symbol="true" />

<item itemtype="Clock" CircId="Clock-4" mainComp="false" Show_id="false" Show_Val="true" Pos="-476,-304" rotation="0" hflip="1" vflip="1" label="Clock-4" idLabPos="-64,-24" labelrot="0" valLabPos="-16,8" valLabRot="0" Out="true" Running="true" Voltage="5 V" Freq="6000 Hz" Always_On="false" />

<item itemtype="Fixed Voltage" CircId="Fixed Voltage-6" mainComp="false" Show_id="false" Show_Val="true" Pos="-476,-268" rotation="0" hflip="1" vflip="1" label="Fixed Voltage-6" idLabPos="-64,-24" labelrot="0" valLabPos="-16,8" valLabRot="0" Out="false" Voltage="5 V" />

<item itemtype="FreqMeter" CircId="Frequencimeter-8" mainComp="false" Show_id="false" Show_Val="false" Pos="-380,-372" rotation="0" hflip="1" vflip="1" label="Frequencimeter-8" idLabPos="-32,-24" labelrot="0" valLabPos="0,0" valLabRot="0" Filter="0.1 V" />

<item itemtype="FreqMeter" CircId="Frequencimeter-12" mainComp="false" Show_id="false" Show_Val="false" Pos="-272,-340" rotation="0" hflip="1" vflip="1" label="Frequencimeter-12" idLabPos="-32,-24" labelrot="0" valLabPos="0,0" valLabRot="0" Filter="0.1 V" />

<item itemtype="Probe" CircId="Probe-16" mainComp="false" Show_id="false" Show_Val="true" Pos="-196,-304" rotation="-45" hflip="1" vflip="1" label="Probe-16" idLabPos="16,-16" labelrot="45" valLabPos="16,0" valLabRot="45" ShowVolt="true" Threshold="2.5 V" />

<item itemtype="FreqMeter" CircId="Frequencimeter-18" mainComp="false" Show_id="false" Show_Val="false" Pos="-276,-308" rotation="0" hflip="1" vflip="1" label="Frequencimeter-18" idLabPos="-32,-24" labelrot="0" valLabPos="0,0" valLabRot="0" Filter="0.1 V" />

<item itemtype="FreqMeter" CircId="Frequencimeter-20" mainComp="false" Show_id="false" Show_Val="false" Pos="-244,-256" rotation="0" hflip="1" vflip="1" label="Frequencimeter-20" idLabPos="-32,-24" labelrot="0" valLabPos="0,0" valLabRot="0" Filter="0.1 V" />

<item itemtype="Node" CircId="Node-10" mainComp="false" Pos="-448,-304" />

<item itemtype="Node" CircId="Node-14" mainComp="false" Pos="-344,-340" />

<item itemtype="Node" CircId="Node-22" mainComp="false" Pos="-284,-288" />

<item itemtype="Connector" uid="Connector-2" startpinid="74XX57-1-QA" endpinid="Node-14-0" pointList="-364,-304,-344,-304,-344,-340" />

<item itemtype="Connector" uid="Connector-5" startpinid="Clock-4-outnod" endpinid="Node-10-0" pointList="-460,-304,-448,-304" />

<item itemtype="Connector" uid="Connector-7" startpinid="Fixed Voltage-6-outnod" endpinid="74XX57-1-RES" pointList="-460,-268,-412,-268,-412,-288" />

<item itemtype="Connector" uid="Connector-9" startpinid="Frequencimeter-8-lPin" endpinid="Node-10-1" pointList="-420,-372,-448,-372,-448,-304" />

<item itemtype="Connector" uid="Connector-11" startpinid="Node-10-2" endpinid="74XX57-1-CLKA" pointList="-448,-304,-412,-304" />

<item itemtype="Connector" uid="Connector-13" startpinid="Frequencimeter-12-lPin" endpinid="Node-14-1" pointList="-312,-340,-344,-340" />

<item itemtype="Connector" uid="Connector-15" startpinid="Node-14-2" endpinid="74XX57-1-CLKB" pointList="-344,-340,-344,-352,-432,-352,-432,-296,-412,-296" />

<item itemtype="Connector" uid="Connector-17" startpinid="Probe-16-inpin" endpinid="Node-22-0" pointList="-212,-288,-284,-288" />

<item itemtype="Connector" uid="Connector-21" startpinid="Frequencimeter-20-lPin" endpinid="Node-22-1" pointList="-284,-256,-284,-288" />

<item itemtype="Connector" uid="Connector-23" startpinid="Node-22-2" endpinid="74XX57-1-QC" pointList="-284,-288,-364,-288" />

<item itemtype="Connector" uid="Connector-127" startpinid="Frequencimeter-18-lPin" endpinid="74XX57-1-QB" pointList="-316,-308,-328,-308,-328,-296,-364,-296" />

</circuit>