<circuit type="simulide_1.0" stepSize="1000000" stepsPS="1000000" NLsteps="100000" animate="1" >

<item itemtype="Fixed Voltage" CircId="Fixed Volt.-2" mainComp="false" Show_id="true" Show_Val="false" Pos="-324,-140" rotation="0" hflip="1" vflip="1" label="E" idLabPos="-47,-9" labelrot="0" valLabPos="0,0" valLabRot="0" Out="false" Voltage="5 V" />

<item itemtype="Fixed Voltage" CircId="Fixed Volt.-3" mainComp="false" Show_id="true" Show_Val="false" Pos="-324,-108" rotation="0" hflip="1" vflip="1" label="S" idLabPos="-47,-9" labelrot="0" valLabPos="0,0" valLabRot="0" Out="false" Voltage="5 V" />

<item itemtype="Fixed Voltage" CircId="Fixed Volt.-4" mainComp="false" Show_id="true" Show_Val="false" Pos="-324,-172" rotation="0" hflip="1" vflip="1" label="R" idLabPos="-47,-9" labelrot="0" valLabPos="0,0" valLabRot="0" Out="false" Voltage="5 V" />

<item itemtype="Or Gate" CircId="Or Gate-5" mainComp="false" Show_id="false" Show_Val="false" Pos="-228,-116" rotation="0" hflip="1" vflip="1" label="Or Gate-5" idLabPos="0,-24" labelrot="0" valLabPos="0,0" valLabRot="0" Num_Inputs="2 _Inputs" Inverted="true" Open_Collector="false" Input_High_V="2.5 V" Input_Low_V="2.5 V" Input_Imped="1e+20 Ω" Out_High_V="5 V" Out_Low_V="0 V" Out_Imped="50 Ω" rndPD="false" Tpd_ps="10000 ps" Tr_ps="3000 ps" Tf_ps="4000 ps" />

<item itemtype="Or Gate" CircId="Or Gate-6" mainComp="false" Show_id="false" Show_Val="false" Pos="-228,-164" rotation="0" hflip="1" vflip="1" label="Or Gate-6" idLabPos="0,-24" labelrot="0" valLabPos="0,0" valLabRot="0" Num_Inputs="2 _Inputs" Inverted="true" Open_Collector="false" Input_High_V="2.5 V" Input_Low_V="2.5 V" Input_Imped="1e+20 Ω" Out_High_V="5 V" Out_Low_V="0 V" Out_Imped="50 Ω" rndPD="true" Tpd_ps="10000 ps" Tr_ps="3000 ps" Tf_ps="4000 ps" />

<item itemtype="And Gate" CircId="And Gate-7" mainComp="false" Show_id="false" Show_Val="false" Pos="-268,-112" rotation="0" hflip="1" vflip="1" label="And Gate-7" idLabPos="0,-24" labelrot="0" valLabPos="0,0" valLabRot="0" Num_Inputs="2 _Inputs" Inverted="false" Open_Collector="false" Input_High_V="2.5 V" Input_Low_V="2.5 V" Input_Imped="1e+20 Ω" Out_High_V="5 V" Out_Low_V="0 V" Out_Imped="50 Ω" rndPD="false" Tpd_ps="10000 ps" Tr_ps="3000 ps" Tf_ps="4000 ps" />

<item itemtype="And Gate" CircId="And Gate-8" mainComp="false" Show_id="false" Show_Val="false" Pos="-268,-168" rotation="0" hflip="1" vflip="1" label="And Gate-8" idLabPos="0,-24" labelrot="0" valLabPos="0,0" valLabRot="0" Num_Inputs="2 _Inputs" Inverted="false" Open_Collector="false" Input_High_V="2.5 V" Input_Low_V="2.5 V" Input_Imped="1e+20 Ω" Out_High_V="5 V" Out_Low_V="0 V" Out_Imped="50 Ω" rndPD="false" Tpd_ps="10000 ps" Tr_ps="3000 ps" Tf_ps="4000 ps" />

<item itemtype="Probe" CircId="Probe-9" mainComp="false" Show_id="true" Show_Val="false" Pos="-164,-180" rotation="-45" hflip="1" vflip="1" label="Q" idLabPos="14,3" labelrot="45" valLabPos="11,-20" valLabRot="45" ShowVolt="false" Threshold="2.5 V" />

<item itemtype="Probe" CircId="Probe-11" mainComp="false" Show_id="true" Show_Val="false" Pos="-164,-132" rotation="-45" hflip="1" vflip="1" label="Q'" idLabPos="14,1" labelrot="45" valLabPos="-11,3" valLabRot="45" ShowVolt="false" Threshold="2.5 V" />

<item itemtype="Node" CircId="Node-1" mainComp="false" Pos="-292,-140" />

<item itemtype="Node" CircId="Node-10" mainComp="false" Pos="-204,-164" />

<item itemtype="Node" CircId="Node-12" mainComp="false" Pos="-196,-116" />

<item itemtype="Connector" uid="Connector-13" startpinid="And Gate-8-out" endpinid="Or Gate-6-in0" pointList="-252,-168,-244,-168" />

<item itemtype="Connector" uid="Connector-15" startpinid="And Gate-7-out" endpinid="Or Gate-5-in1" pointList="-252,-112,-244,-112" />

<item itemtype="Connector" uid="Connector-17" startpinid="Fixed Volt.-3-outnod" endpinid="And Gate-7-in1" pointList="-308,-108,-284,-108" />

<item itemtype="Connector" uid="Connector-19" startpinid="Fixed Volt.-4-outnod" endpinid="And Gate-8-in0" pointList="-308,-172,-284,-172" />

<item itemtype="Connector" uid="Connector-21" startpinid="And Gate-8-in1" endpinid="Node-1-0" pointList="-284,-164,-292,-164,-292,-140" />

<item itemtype="Connector" uid="Connector-23" startpinid="Fixed Volt.-2-outnod" endpinid="Node-1-1" pointList="-308,-140,-292,-140" />

<item itemtype="Connector" uid="Connector-24" startpinid="Node-1-2" endpinid="And Gate-7-in0" pointList="-292,-140,-292,-116,-284,-116" />

<item itemtype="Connector" uid="Connector-25" startpinid="Or Gate-6-out" endpinid="Node-10-0" pointList="-212,-164,-204,-164" />

<item itemtype="Connector" uid="Connector-27" startpinid="Or Gate-5-out" endpinid="Node-12-0" pointList="-212,-116,-196,-116" />

<item itemtype="Connector" uid="Connector-29" startpinid="Node-10-2" endpinid="Or Gate-5-in0" pointList="-204,-164,-204,-132,-252,-132,-252,-120,-244,-120" />

<item itemtype="Connector" uid="Connector-30" startpinid="Node-10-1" endpinid="Probe-9-inpin" pointList="-204,-164,-180,-164" />

<item itemtype="Connector" uid="Connector-32" startpinid="Node-12-1" endpinid="Probe-11-inpin" pointList="-196,-116,-180,-116" />

<item itemtype="Connector" uid="Connector-31" startpinid="Node-12-2" endpinid="Or Gate-6-in1" pointList="-196,-116,-196,-148,-252,-148,-252,-160,-244,-160" />

</circuit>