<circuit type="simulide_1.0" stepSize="1000000" stepsPS="1000000" NLsteps="100000" animate="0" >

<item itemtype="Subcircuit" CircId="74HC4052-1" mainComp="false" Show_id="true" Show_Val="false" Pos="-296,-292" rotation="0" hflip="1" vflip="1" label="74HC4052-1" idLabPos="0,-20" labelrot="0" valLabPos="0,0" valLabRot="0" Logic_Symbol="true" />

<item itemtype="Probe" CircId="Probe-2" mainComp="false" Show_id="false" Show_Val="true" Pos="-184,-300" rotation="-45" hflip="1" vflip="1" label="Probe-2" idLabPos="16,-16" labelrot="45" valLabPos="16,0" valLabRot="45" ShowVolt="true" Threshold="2.5 V" />

<item itemtype="Voltage Source" CircId="Voltage Source-4" mainComp="false" ShowProp="MaxValue" Show_id="false" Show_Val="true" Pos="-452,-308" rotation="0" hflip="1" vflip="1" label="Voltage Source-4" idLabPos="-40,-80" labelrot="0" valLabPos="-26,10" valLabRot="0" MaxValue="5 V" />

<item itemtype="Voltage Source" CircId="Voltage Source-6" mainComp="false" ShowProp="MaxValue" Show_id="false" Show_Val="true" Pos="-508,-264" rotation="0" hflip="1" vflip="1" label="Voltage Source-6" idLabPos="-40,-80" labelrot="0" valLabPos="-26,10" valLabRot="0" MaxValue="5 V" />

<item itemtype="Probe" CircId="Probe-8" mainComp="false" Show_id="false" Show_Val="true" Pos="-408,-236" rotation="-45" hflip="1" vflip="1" label="Probe-2" idLabPos="16,-16" labelrot="45" valLabPos="16,0" valLabRot="45" ShowVolt="true" Threshold="2.5 V" />

<item itemtype="Probe" CircId="Probe-10" mainComp="false" Show_id="false" Show_Val="true" Pos="-356,-256" rotation="-45" hflip="1" vflip="1" label="Probe-2" idLabPos="16,-16" labelrot="45" valLabPos="16,0" valLabRot="45" ShowVolt="true" Threshold="2.5 V" />

<item itemtype="Voltage Source" CircId="Voltage Source-12" mainComp="false" ShowProp="MaxValue" Show_id="false" Show_Val="true" Pos="-140,-256" rotation="0" hflip="1" vflip="1" label="Voltage Source-4" idLabPos="-40,-80" labelrot="0" valLabPos="-26,10" valLabRot="0" MaxValue="5 V" />

<item itemtype="Fixed Voltage" CircId="Fixed Voltage-14" mainComp="false" Show_id="true" Show_Val="false" Pos="-448,-196" rotation="0" hflip="1" vflip="1" label="S0" idLabPos="-50,-6" labelrot="0" valLabPos="-16,8" valLabRot="0" Out="false" Voltage="5 V" />

<item itemtype="Fixed Voltage" CircId="Fixed Voltage-16" mainComp="false" Show_id="true" Show_Val="false" Pos="-448,-180" rotation="0" hflip="1" vflip="1" label="S1" idLabPos="-50,-6" labelrot="0" valLabPos="-16,8" valLabRot="0" Out="true" Voltage="5 V" />

<item itemtype="Fixed Voltage" CircId="Fixed Voltage-18" mainComp="false" Show_id="true" Show_Val="false" Pos="-436,-136" rotation="0" hflip="1" vflip="1" label="!E" idLabPos="-50,-6" labelrot="0" valLabPos="-16,8" valLabRot="0" Out="true" Voltage="5 V" />

<item itemtype="Connector" uid="Connector-3" startpinid="Probe-2-inpin" endpinid="74HC4052-1-1Z" pointList="-200,-284,-256,-284" />

<item itemtype="Connector" uid="Connector-5" startpinid="Voltage Source-4-outPin" endpinid="74HC4052-1-1Y0" pointList="-424,-292,-424,-308,-304,-308,-304,-284" />

<item itemtype="Connector" uid="Connector-7" startpinid="Voltage Source-6-outPin" endpinid="74HC4052-1-1Y1" pointList="-480,-248,-480,-264,-380,-264,-380,-276,-304,-276" />

<item itemtype="Connector" uid="Connector-9" startpinid="Probe-8-inpin" endpinid="74HC4052-1-2Y3" pointList="-424,-220,-304,-220" />

<item itemtype="Connector" uid="Connector-11" startpinid="Probe-10-inpin" endpinid="74HC4052-1-2Y2" pointList="-372,-240,-372,-228,-304,-228" />

<item itemtype="Connector" uid="Connector-13" startpinid="Voltage Source-12-outPin" endpinid="74HC4052-1-2Z" pointList="-112,-240,-112,-216,-220,-216,-220,-244,-256,-244" />

<item itemtype="Connector" uid="Connector-15" startpinid="Fixed Voltage-14-outnod" endpinid="74HC4052-1-S0" pointList="-432,-196,-368,-196,-368,-204,-304,-204" />

<item itemtype="Connector" uid="Connector-17" startpinid="Fixed Voltage-16-outnod" endpinid="74HC4052-1-S1" pointList="-432,-180,-360,-180,-360,-196,-304,-196" />

<item itemtype="Connector" uid="Connector-19" startpinid="Fixed Voltage-18-outnod" endpinid="74HC4052-1-!E" pointList="-420,-136,-304,-136,-304,-188" />

</circuit>