<circuit type="simulide_1.0" stepSize="1000000" stepsPS="1000000" NLsteps="100000" animate="0" >

<item itemtype="TextComponent" CircId="TextComponent-412" mainComp="false" Show_id="false" Show_Val="false" Pos="-244,-172" rotation="0" hflip="1" vflip="1" label="TextComponent-412" idLabPos="-16,-24" labelrot="0" valLabPos="0,0" valLabRot="0" Margin="5 _Pixels" Border="1 _Pixels" Opacity="1" Font="Helvetica [Cronyx]" Font_Size="10 _Pixels" Fixed_Width="true" Text="PinOut:&#xa;1 - Power&#xa;2 - Blank (active Low)&#xa;3 - NC&#xa;4 - Count Out (divide by 10)&#xa;5 - Power&#xa;6 - Reset (active High)&#xa;7 - Count in (active L to H)&#xa;8 - Gnd&#xa;9 - Dot&#xa;10- NC&#xa;" />

<item itemtype="Subcircuit" CircId="K490IP1-1" mainComp="false" Show_id="true" Show_Val="false" Pos="-448,-180" rotation="0" hflip="1" vflip="1" label="K490IP1-1" idLabPos="0,-20" labelrot="0" valLabPos="17,31" valLabRot="-90" Logic_Symbol="false" />

<item itemtype="Subcircuit" CircId="K490IP1-88" mainComp="false" Show_id="true" Show_Val="false" Pos="-352,-180" rotation="0" hflip="1" vflip="1" label="K490IP1-1" idLabPos="0,-20" labelrot="0" valLabPos="17,31" valLabRot="-90" Logic_Symbol="false" />

<item itemtype="Fixed Voltage" CircId="Fixed Voltage-176" mainComp="false" Show_id="true" Show_Val="false" Pos="-520,-164" rotation="0" hflip="1" vflip="1" label="Blanc = Low" idLabPos="-37,-24" labelrot="0" valLabPos="-16,8" valLabRot="0" Out="true" Voltage="5 V" />

<item itemtype="Fixed Voltage" CircId="Fixed Voltage-180" mainComp="false" Show_id="true" Show_Val="false" Pos="-524,-88" rotation="0" hflip="1" vflip="1" label="Reset = Hi" idLabPos="-37,-24" labelrot="0" valLabPos="-16,8" valLabRot="0" Out="false" Voltage="5 V" />

<item itemtype="Clock" CircId="Clock-185" mainComp="false" Show_id="false" Show_Val="true" Pos="-520,-52" rotation="0" hflip="1" vflip="1" label="Clock-185" idLabPos="-64,-24" labelrot="0" valLabPos="-16,8" valLabRot="0" Out="true" Running="true" Voltage="5 V" Freq="2 Hz" Always_On="false" />

<item itemtype="Fixed Voltage" CircId="Fixed Voltage-187" mainComp="false" Show_id="true" Show_Val="false" Pos="-332,-20" rotation="0" hflip="1" vflip="1" label="Dot" idLabPos="-8,-23" labelrot="0" valLabPos="-16,8" valLabRot="0" Out="true" Voltage="5 V" />

<item itemtype="Fixed Voltage" CircId="Fixed Voltage-189" mainComp="false" Show_id="true" Show_Val="false" Pos="-436,-20" rotation="0" hflip="1" vflip="1" label="Dot" idLabPos="-8,-22" labelrot="0" valLabPos="-16,8" valLabRot="0" Out="true" Voltage="5 V" />

<item itemtype="Node" CircId="Node-178" mainComp="false" Pos="-468,-164" />

<item itemtype="Node" CircId="Node-182" mainComp="false" Pos="-400,-88" />

<item itemtype="Connector" uid="Connector-175" startpinid="K490IP1-88-Bl" endpinid="Node-178-0" pointList="-360,-164,-380,-164,-380,-100,-468,-100,-468,-164" />

<item itemtype="Connector" uid="Connector-177" startpinid="Fixed Voltage-176-outnod" endpinid="Node-178-1" pointList="-504,-164,-468,-164" />

<item itemtype="Connector" uid="Connector-179" startpinid="Node-178-2" endpinid="K490IP1-1-Bl" pointList="-468,-164,-456,-164" />

<item itemtype="Connector" uid="Connector-181" startpinid="Fixed Voltage-180-outnod" endpinid="Node-182-0" pointList="-508,-88,-400,-88" />

<item itemtype="Connector" uid="Connector-183" startpinid="Node-182-2" endpinid="K490IP1-1-R" pointList="-400,-88,-400,-140" />

<item itemtype="Connector" uid="Connector-184" startpinid="Node-182-1" endpinid="K490IP1-88-R" pointList="-400,-88,-304,-88,-304,-140" />

<item itemtype="Connector" uid="Connector-186" startpinid="Clock-185-outnod" endpinid="K490IP1-88-C" pointList="-504,-52,-292,-52,-292,-148,-304,-148" />

<item itemtype="Connector" uid="Connector-188" startpinid="Fixed Voltage-187-outnod" endpinid="K490IP1-88-H" pointList="-316,-20,-284,-20,-284,-164,-304,-164" />

<item itemtype="Connector" uid="Connector-190" startpinid="Fixed Voltage-189-outnod" endpinid="K490IP1-1-H" pointList="-420,-20,-388,-20,-388,-164,-400,-164" />

<item itemtype="Connector" uid="Connector-191" startpinid="K490IP1-88-Co" endpinid="K490IP1-1-C" pointList="-360,-148,-400,-148" />

</circuit>