<circuit type="simulide_1.0" stepSize="1000000" stepsPS="1000000" NLsteps="100000" animate="1" >

<item itemtype="Amperimeter" CircId="Amperimeter-9" mainComp="false" Show_id="false" Show_Val="false" Pos="-340,-244" rotation="0" hflip="1" vflip="1" label="Amperimeter-24" idLabPos="-12,-24" labelrot="0" valLabPos="-20,-22" valLabRot="0" SwitchPins="false" />

<item itemtype="Ground" CircId="Ground (0 V)-8" mainComp="false" Show_id="false" Show_Val="false" Pos="-172,-44" rotation="0" hflip="1" vflip="1" label="Ground (0 V)-22" idLabPos="-16,-24" labelrot="0" valLabPos="0,0" valLabRot="0" />

<item itemtype="Resistor" CircId="Resistor-7" mainComp="false" ShowProp="Resistance" Show_id="false" Show_Val="true" Pos="-172,-116" rotation="90" hflip="1" vflip="1" label="Resistor-20" idLabPos="-12,-24" labelrot="0" valLabPos="-16,6" valLabRot="0" Resistance="100 Ω" />

<item itemtype="Rail" CircId="Rail.-6" mainComp="false" ShowProp="Voltage" Show_id="false" Show_Val="true" Pos="-332,-332" rotation="0" hflip="1" vflip="1" label="Rail.-18" idLabPos="-64,-24" labelrot="0" valLabPos="-16,8" valLabRot="0" Voltage="5 V" />

<item itemtype="BJT" CircId="BJT-5" mainComp="false" Show_id="false" Show_Val="false" Pos="-244,-196" rotation="0" hflip="1" vflip="-1" label="BJT-6" idLabPos="-16,-24" labelrot="0" valLabPos="0,0" valLabRot="0" PNP="true" Gain="100" />

<item itemtype="Amperimeter" CircId="Amperimeter-4" mainComp="false" Show_id="false" Show_Val="false" Pos="-180,-188" rotation="0" hflip="1" vflip="1" label="Amperimeter-4" idLabPos="-12,-24" labelrot="0" valLabPos="-20,-22" valLabRot="0" SwitchPins="false" />

<item itemtype="Voltage Source" CircId="Volt. Source-3" mainComp="false" ShowProp="MaxValue" Show_id="false" Show_Val="true" Pos="-440,-212" rotation="0" hflip="1" vflip="1" label="Volt. Source-3" idLabPos="-16,-24" labelrot="0" valLabPos="-8,-42" valLabRot="0" MaxValue="5 V" />

<item itemtype="Resistor" CircId="Resistor-2" mainComp="false" ShowProp="Resistance" Show_id="false" Show_Val="true" Pos="-380,-196" rotation="0" hflip="1" vflip="1" label="Resistor-2" idLabPos="-12,-24" labelrot="0" valLabPos="-11,10" valLabRot="0" Resistance="1 kΩ" />

<item itemtype="Probe" CircId="Probe-1" mainComp="false" Show_id="false" Show_Val="true" Pos="-292,-212" rotation="-45" hflip="1" vflip="1" label="Probe-1" idLabPos="16,-16" labelrot="45" valLabPos="16,0" valLabRot="45" ShowVolt="true" Threshold="2.5 V" />

<item itemtype="Probe" CircId="Probe-10" mainComp="false" Show_id="false" Show_Val="true" Pos="-388,-212" rotation="-45" hflip="1" vflip="1" label="Probe-10" idLabPos="16,-16" labelrot="45" valLabPos="16,0" valLabRot="45" ShowVolt="true" Threshold="2.5 V" />

<item itemtype="Connector" uid="Connector-10" startpinid="BJT-5-collector" endpinid="Amperimeter-4-lPin" pointList="-236,-180,-236,-156,-188,-156,-188,-172" />

<item itemtype="Connector" uid="Connector-12" startpinid="Volt. Source-3-outPin" endpinid="Resistor-2-lPin" pointList="-412,-196,-396,-196" />

<item itemtype="Connector" uid="Connector-14" startpinid="Rail.-6-outnod" endpinid="BJT-5-emiter" pointList="-316,-332,-236,-332,-236,-212" />

<item itemtype="Connector" uid="Connector-16" startpinid="Amperimeter-4-rPin" endpinid="Resistor-7-lPin" pointList="-172,-172,-172,-132" />

<item itemtype="Connector" uid="Connector-18" startpinid="Ground (0 V)-8-Gnd" endpinid="Resistor-7-rPin" pointList="-172,-60,-172,-100" />

<item itemtype="Connector" uid="Connector-20" startpinid="Resistor-2-rPin" endpinid="Amperimeter-9-lPin" pointList="-364,-196,-348,-196,-348,-228" />

<item itemtype="Connector" uid="Connector-22" startpinid="Amperimeter-9-rPin" endpinid="BJT-5-base" pointList="-332,-228,-332,-196,-260,-196" />

</circuit>