# Compilation Report

Compiler Version (DD/MM/YYYY): 0.96.<<>> 2016-12-14

## Chip resource usage:

Chip Model: 18F4550

Program Memory: 1783/16384 words (10.88%)

RAM: 43/2048 bytes (2.1%)

## RAM Allocation

## Subroutines

Name | Code Size (lines) | Compiled Size (words) | Outgoing calls
--- | --- | --- | ---
Main | 43 | 66 | SYSCOMPLESSTHAN16(4), INITGLCD_KS0108(33), Delay_MS(2), GLCDBMPLOAD(2), GLCDCLS_KS0108(2), INITSYS(1)
GLCDBMPLOAD | 106 | 622 | SYSCOMPEQUAL(1), SYSDIVSUB(4), SYSCOMPLESSTHAN(8), SYSCOMPEQUAL16(15), PSET_KS0108(4), GLCDWRITEBYTE_KS0108(3)
INITGLCD_KS0108 | 25 | 44 | Delay_MS(2), GLCDCLS_KS0108(1), GLCDWRITEBYTE_KS0108(2)
GLCDCLS_KS0108 | 21 | 46 | GLCDWRITEBYTE_KS0108(3)
PSET_KS0108 | 48 | 91 | SYSDIVSUB(1), GLCDREADBYTE_KS0108(2), GLCDWRITEBYTE_KS0108(4)
GLCDWRITEBYTE_KS0108 | 45 | 74 | GLCDREADBYTE_KS0108(1)
GLCDREADBYTE_KS0108 | 21 | 46 |
INITSYS | 579 | 17 |
SYSDIVSUB | 48 | 22 |
SYSCOMPEQUAL | 20 | 5 |
SYSCOMPEQUAL16 | 34 | 9 |
SYSCOMPLESSTHAN | 23 | 5 |
SYSCOMPLESSTHAN16 | 38 | 14 |
Delay_MS | 0 | 18 |
GLCDTABLE1 | 0 | 265 |
GLCDTABLE1_H | 0 | 23 |
GLCDTABLE2 | 0 | 348 |
GLCDTABLE2_H | 0 | 23 |
GLCDTABLE3 | 0 | 15 |
GLCDTABLE4 | 0 | 15 |
GLCDTABLE5 | 0 | 15 |